Andante-16                 [ Digital Mixer ]

1. 제 품 특 징

- 16 in 8 out 디지털 믹서

- Matrix, Automix, EQ, Delay, Gate 등의 필요한 모든 프로세서 탑재

- 선택 가능한 모든 입력단과 매트릭스 출력단

- 233m 까지 조절 가능한 딜레이

- 모든 프로세서를 셋업 가능한 개방형 PC 소프트웨어

- 프론트 판넬에서의 조작이 용이한 저장, 호출 가능한 20개 프리셋

- 제어 장치에 의해 시스템 통합 가능한 RS-232 시리얼 포트와 프로토콜

- 복잡한 시스템을 직관적으로 쉽게 조작 가능한 편리성

2. 제 품 규 격

- 입력	: 14 XLR + 2 XLR/RCA

Sensitivity per input: Mic/Line

Digitally controlled phantom power per input: 48V

THD input to output (all ganin settings): <=0,01%

- 출력	: 6 XLR + 2 XLR/RCA

THD input to output (all gain settings): <= 0.01%

- 디지털 시그널 프로세싱

<inputs >

: 3 parametric EQs per Input (peaking type)

Highpass Filter 160 Hz/12 dB per octave on every input

Gate/compressor/limiter per Input

<Outputs>

: Graphic EQ per line output: 31 band (1/3 oct)

4 parametriic EQs per line output (peaking type)

Gate/compressor/limiter per output

Delay per line output 233 m (679 ms)

Phase reverse per line output

- Input/Output Routing Matrix Size of matrix: 16 In / 8 Out

Individual volume (fader) per crosspoint

- Automix	: Automatic mixing function

Automatic mixing function simultaneous channels selectable

- General	: Sample frequency: 48 kHz

- 유저 인터페이스	: Master volume (common level for all outputs)

accessible via front panel

20 presets accessible via front panel

Presets include analog input gain and phantompower setting

Individual input and output volume setting accessible via front panel

Peak- and signal indicator per input channel on front panel

DSP-parameters accessible via frontpanel,

PC/Notebook-USB-Interface

Preset load from and save to file (PC software)

External remote control via RS 232

(see serial protocol description)

Switchable user access protection

- 제품사이즈(WHD)	: 483 x 88 x 260mm (with connector 320mm)

- 무게	: 5.2 kg

- 용도	: 회의실, 강당, 종교시설, 관공서, 테마파크, 학교, 기업,

인스톨 사운드용