ES1.0                                        [ 3-WAY Loud Speaker ]

1. 제 품 특 징

- 연속출력 131dB, 피크출력 134dB(ES1.0 only)

- 90° x 40° Rotatable 디자인

- 매우 낮은 디스토션과 확장된 주파수 레스폰스 특성을 가능하게 하는 1.75" 티타늄

컴프레션 드라이버와 컴플렉스 지오메트리 페이즈 플러그의 완벽한 하모니

- 6" 미드레인지 드라이버와 1.75"(44mm) 보이스코일과 네오디뮴 마그네트 구조로 고출력에서

도 낮은 디스토션의 퍼포먼스 제공

- 3 Way Active 디자인 - EPAK2500/R 파워 앰프를 통해 Low mid(12")-600w, Mid(6")-200w,

Hi(1.75")-100w 공급

- 정교한 수평 수직 스택을 위해 3면에 비대칭 배치된 하이 임팩트 저마찰 인슐레이터

- 손쉬운 취급과 운반을 위한 독자적인 핸들 디자인

- 폴 마운팅 어플리케이션을 위한 Top hat, 24개의 서스펜션 플라잉 포인트

- 전천후 방수 기능과 스페셜 컬러 주문 가능

- 정교한 수평 수직 스택을 위해 3면에 비대칭 배치된 하이 임팩트 저마찰 인슐레이터

2. 제 품 규 격

- 주파수 응답	: 130Hz ~ 20kHz (-3dB Point)

- 드라이버 구성	: HF : 1 x 1" / MF : 1 x 6" / LF : 1 x 12"

- 앰프 권장 요구사항	: HF : 100W / MF : 200W / LF : 600W (EPAK2500/R앰프 권장)

- 임피던스	: HF : 8Ω / MF : 8Ω / LF : 16Ω

- 최대 출력 감도	: 134dB Peak

- 크로스오버 포인트	: 130Hz, 500Hz, 2.5KHz

- 커버리지	: 90˚H x 40˚V Rotable

- 커넥터	: AP-6

- 인클로저 재질	: Baltic birch

- 리깅 포인트	: 8 x M10 suspension points, Hole Cup, flybars,

horizontal and vertical brackets

- 제품 사이즈 (HWD)	: 700 x 450 x 450mm

- 무게	: 34kg

- 악세서리	: Additional arms for Bracket, Cart ES1.0, Cart Wheels,

COVER ES1.0, ES Downfill Bracket, ES1.0 Full grille,

Flybar and Bracket for ES Systems,

Horizontal Bracket for ES1.0, Speaker pole-universal,

Vertical Bracket for ES1.0,

Set of M10 x 50 closed end bolts for 6mm quick lock pin